,_DistributedBy##OTHER##,_CurrentRevision##OTHER##,_CreatedBy##OTHER##,_BimSpecGuid##OTHER##,_BSBibleVersion##OTHER##,_Author##OTHER##,Water_Treatment_Required##OTHER##,Water_Content##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDescription##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type##OTHER##,Turndown_Ratio##OTHER##,Total top to bottom clearance##LENGTH##MILLIMETERS,Total lleft to right clearance##LENGTH##MILLIMETERS,Total front to back clearance##LENGTH##MILLIMETERS,Supply_Phase##OTHER##,SupplySide##LENGTH##MILLIMETERS,SupplyHeight##LENGTH##MILLIMETERS,SupplyReturnLenght##LENGTH##MILLIMETERS,SupplyDiameter##LENGTH##MILLIMETERS,Starting_Current##OTHER##,Sound_Pressure_Level##OTHER##,Silencer##OTHER##,Shipping_Weight##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,Safety_Valve_Connection_Type##OTHER##,Safety_Valve_Connection_Size##OTHER##,ReturnSide##LENGTH##MILLIMETERS,ReturnHeight##LENGTH##MILLIMETERS,ReturnDiameter##LENGTH##MILLIMETERS,Referenced_Standard##OTHER##,Rated_Output##OTHER##,Rated_Criteria##OTHER##,Product_Range##OTHER##,Product_Model_Number##OTHER##,Product_Literature##OTHER##,Manufacturer##OTHER##,Primary_Fuel##OTHER##,Overall_Width##LENGTH##MILLIMETERS,Overall_Length##LENGTH##MILLIMETERS,Overall_Height##LENGTH##MILLIMETERS,Optional_Fuel##OTHER##,Description##OTHER##,Oil_Consumption_rate##OTHER##,Nominal_Oil_Inlet_Pressure##OTHER##,Nominal_Gas_Inlet_Pressure##OTHER##,NominalLength##OTHER##,NominalHeight##OTHER##,NominalDepth##OTHER##,NOx_Emissions##OTHER##,NBSReference##OTHER##,NBSOfficeMasterTag##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,Mounting##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Minimum_Power_Consumption##OTHER##,Minimum_Operating_Pressure##OTHER##,Minimum_Oil_Inlet_Pressure##OTHER##,Minimum_Gas_Inlet_Pressure##OTHER##,Minimum_Flow_Rate_At_20C_Temperature_Differential##OTHER##,Minimum_Flow_Rate_At_11C_Temperature_Differential##OTHER##,Maximum_Power_Consumption##OTHER##,Maximum_Operating_Pressure##OTHER##,Maximum_Oil_Inlet_Pressure##OTHER##,Maximum_Gas_Inlet_Pressure##OTHER##,Material##OTHER##,Manufacturer_Website##OTHER##,Manufacturer_2##OTHER##,ManufactureName##OTHER##,Assembly Code##OTHER##,Interlocks##OTHER##,InstallationDate##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,IP_Rating##OTHER##,IK_Rating##OTHER##,Hydraulic_Resistance_at_20C_temperature_differential##OTHER##,Hydraulic_Resistance_at_11C_temperature_differential##OTHER##,HeaterOperation##OTHER##,Heat_Exchanger_Material##OTHER##,Gross_Weight##OTHER##,Gas_Consumption_rate##OTHER##,GasSide##LENGTH##MILLIMETERS,GasLenght##LENGTH##MILLIMETERS,GasHeight##LENGTH##MILLIMETERS,GasDiameter##LENGTH##MILLIMETERS,Fuse_Rating##OTHER##,Full_Load_Current##OTHER##,Fuel_Connection_Type##OTHER##,Fuel_Connection_Size##OTHER##,Frequency##OTHER##,Flue_or_Air_Intake_Classification##OTHER##,Flue_Connection_Size##OTHER##,FlueGasSide##LENGTH##MILLIMETERS,FlueGasCenter##LENGTH##MILLIMETERS,FlueGasHeight##LENGTH##MILLIMETERS,FlueGasDiameter##LENGTH##MILLIMETERS,Flow_and_Return_Connection_Type##OTHER##,Flow_and_Return_Connection_Size##OTHER##,Finish##OTHER##,External_Material##OTHER##,ExpectedLife##OTHER##,Erp_Seasonal_Efficiency##OTHER##,ErP_Rated_Efficiency_at_Part_Load##OTHER##,ErP_Rated_Efficiency_at_Full_Load##OTHER##,ErP_Energy_Label##OTHER##,DurationUnit##OTHER##,Drain_Connection_Type##OTHER##,Drain_Connection_Size##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Control_Type##OTHER##,Configuration##OTHER##,Condensate_Drain_Type##OTHER##,Condensate_Drain_Size##OTHER##,CondensateSide##LENGTH##MILLIMETERS,CondensateLenght##LENGTH##MILLIMETERS,CondensateHeight##LENGTH##MILLIMETERS,Condensate_Drain_Diameter##LENGTH##MILLIMETERS,Colour##OTHER##,Clerance zone visibility##OTHER##,ClassifcationValue##OTHER##,ClassifcationName##OTHER##,CE_Approval##OTHER##,Burner_Control_Type##OTHER##,Building_Regulations_Seasonal_Efficiency##OTHER##,BarCode##OTHER##,BMS_Links##OTHER##,BIMObjectName##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Air_Inlet_Connection_Size##OTHER##,AirInletSide##LENGTH##MILLIMETERS,AirInletHeight##LENGTH##MILLIMETERS,Air_Inlet_Connection_Diameter##LENGTH##MILLIMETERS,Access_Clearance_Top##LENGTH##MILLIMETERS,Access_Clearance_Right##LENGTH##MILLIMETERS,Access_Clearance_Left##LENGTH##MILLIMETERS,Access_Clearance_Front##LENGTH##MILLIMETERS,Access_Clearance_Bottom##LENGTH##MILLIMETERS,Access_Clearance_Rear##LENGTH##MILLIMETERS,BoilerWidth##LENGTH##MILLIMETERS,BoilerHeight##LENGTH##MILLIMETERS,BoilerDepth##LENGTH##MILLIMETERS,AirInletLenght##LENGTH##MILLIMETERS
Nesta 300 FS,,1,www.myaic.eu,0,16,DaPr,Yes,75 liters,,info@myaic.eu,years,0,,230.000000000000,www.myaic.eu,Space heating,,1924.000000000001,1648.000000000000,2276.000000000000,1,534.000000000000,1098.000000000000,793.000000000000,76.100000000000,n/a,,0,305 kg,Rectangular (Vertical),0,Threaded,G1"",152.000000000000,361.000000000000,76.100000000000,EN 15502-1/EN 15502-2-1,300kW,80/60,Nesta FS,N 300 FS,https://myaic.eu/downloads,AIC Europe BV,Gas - NG,648.000000000000,890.000000000000,1524.000000000000,Gas - LPG,A high efficiency condensing boiler; perfect for single or multiple boiler installations in medium to large buildings including schools; hotels; care homes; offices and commercial buildings.,0,0,20 mbar,648,1524,890,24,90-40-05/340,n/a,AIC_GasFiredCondensingBoiler,,n/a,Floor Standing,Nesta FS,N 300 FS,N 300 FS,34 W,0.8 bar,0,17 bar,3.11 l/s,n/a,410 W,6 bar,0,25 bar,Aluminium; steel; stainless steel;  polymers,www.myaic.eu,AIC Europe BV,AIC Europe BV,,Yes,,Pset_BoilerTypeCommon,IfcBoilerType,IPX4D,n/a,30.31 mbar,n/a,Condensing,Stainless Steel,367,,471.000000000000,759.000000000000,1313.000000000000,33.700000000000,6.3 A,n/a,Threaded,G1"",50 Hz,B23; B23P; C43; C53; C63; C83,180 mm,334.000000000000,104.000000000000,98.000000000000,180.000000000000,Threaded,G 2 1/2"",Painted,Aluminium,,93%,97.39 %,87.71 %,0,years,Threaded,G 1"",,info@myaic.eu,Weather compensating; Optimised Start/Stop; On/Off,Single boiler,Plain,25mm,128.000000000000,700.000000000000,141.000000000000,25.000000000000,grey,1,Pr_60_60_08_34,Uniclass2015,Yes,Modulating,n/a,,Yes,AIC_Boiler_Nesta_FS_300,Fixed,,125mm,167.000000000000,1324.000000000000,125.000000000000,400.000000000000,500.000000000000,500.000000000000,1000.000000000000,0.000000000000,500.000000000000,648.000000000000,1524.000000000000,681.000000000000,721.000000000000
