,_DistributedBy##OTHER##,_CurrentRevision##OTHER##,_CreatedBy##OTHER##,_BimSpecGuid##OTHER##,_BSBibleVersion##OTHER##,_Author##OTHER##,Water_Treatment_Required##OTHER##,Water_Content##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDescription##OTHER##,Voltage##OTHER##,URL##OTHER##,Type##OTHER##,Turndown_Ratio##OTHER##,Supply_Phase##OTHER##,Sound_Pressure_Level##OTHER##,Shipping_Weight##OTHER##,Shape##OTHER##,Safety_Valve_Connection_Type##OTHER##,Safety_Valve_Connection_Size##OTHER##,ReferencedStandard##OTHER##,Rated_Output##OTHER##,Rated_Criteria##OTHER##,Product_Range##OTHER##,Product_Model_Number##OTHER##,Product_Literature##OTHER##,Primary_Fuel##OTHER##,Optional_Fuel##OTHER##,Nominal_Gas_Inlet_Pressure##OTHER##,NominalLength##OTHER##,NominalHeight##OTHER##,NominalDepth##OTHER##,NOx_Emissions##OTHER##,NBSReference##OTHER##,NBSOfficeMasterTag##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,Mounting##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Minimum_Power_Consumption##OTHER##,Minimum_Operating_Pressure##OTHER##,Minimum_Gas_Inlet_Pressure##OTHER##,Minimum_Flow_Rate_At_20C_Temperature_Differential##OTHER##,Maximum_Power_Consumption##OTHER##,Maximum_Operating_Pressure##OTHER##,Maximum_Gas_Inlet_Pressure##OTHER##,Material##OTHER##,Manufacturer_Website##OTHER##,Manufacturer##OTHER##,ManufactureName##OTHER##,Interlocks##OTHER##,InstallationDate##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,IP_Rating##OTHER##,Hydraulic_Resistance_at_20C_temperature_differential##OTHER##,HeaterOperation##OTHER##,Heat_Exchanger_Material##OTHER##,Gross_Weight##OTHER##,Gas_Consumption_rate##OTHER##,Fuse_Rating##OTHER##,Full_Load_Current##OTHER##,Fuel_Connection_Type##OTHER##,Fuel_Connection_Size##OTHER##,Frequency##OTHER##,Flue_or_Air_Intake_Classification##OTHER##,Flue_Connection_Size##OTHER##,FlueGasOffset##LENGTH##MILLIMETERS,FlueGasLength##LENGTH##MILLIMETERS,FlueGasCenter##LENGTH##MILLIMETERS,Flow_and_Return_Connection_Type##OTHER##,Flow_and_Return_Connection_Size##OTHER##,Finish##OTHER##,External_Material##OTHER##,ExpectedLife##OTHER##,Erp_Seasonal_Efficiency##OTHER##,ErP_Rated_Efficiency_at_Part_Load##OTHER##,ErP_Rated_Efficiency_at_Full_Load##OTHER##,ErP_Energy_Label##OTHER##,DurationUnit##OTHER##,Drain_Connection_Type##OTHER##,Drain_Connection_Size##OTHER##,Description##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Control_Type##OTHER##,Configuration##OTHER##,Condensate_Drain_Type##OTHER##,Condensate_Drain_Size##OTHER##,Colour##OTHER##,Clearance from top##LENGTH##MILLIMETERS,Clearance from left##LENGTH##MILLIMETERS,Clearance from front##LENGTH##MILLIMETERS,Clearance from bottom##LENGTH##MILLIMETERS,Clearance from back##LENGTH##MILLIMETERS,Clearance from right##LENGTH##MILLIMETERS,Clearance Zone##OTHER##,ClassifcationValue##OTHER##,ClassifcationName##OTHER##,CE_Approval##OTHER##,Burner_Control_Type##OTHER##,Building_Regulations_Seasonal_Efficiency##OTHER##,Boiler_width##LENGTH##MILLIMETERS,Boiler_depth##LENGTH##MILLIMETERS,SupplyReturnFlangeOffset##LENGTH##MILLIMETERS,SupplyReturnOffset##LENGTH##MILLIMETERS,SupplyReturnLength##LENGTH##MILLIMETERS,SupplyHeight##LENGTH##MILLIMETERS,ReturnHeight##LENGTH##MILLIMETERS,GasOffset##LENGTH##MILLIMETERS,GasInletLength##LENGTH##MILLIMETERS,GasHeight##LENGTH##MILLIMETERS,GasFlangeOffset##LENGTH##MILLIMETERS,CondensateOffset##LENGTH##MILLIMETERS,CondensateHeight##LENGTH##MILLIMETERS,Boiler_height##LENGTH##MILLIMETERS,BarCode##OTHER##,BMS_Links##OTHER##,BIMObjectName##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Air_Inlet_Connection_Size##OTHER##,AirInletTypeC##OTHER##,AirInletTypeB##OTHER##,AirInletOffset##LENGTH##MILLIMETERS,AirInletHeight##LENGTH##MILLIMETERS
Nesta plus 1080 FSW,,0,www.myaic.eu,0,16,DaPr,Yes,600 liters,,info@myaic.eu,years,0,,400,www.myaic.eu,Space heating,,3,86 dB,,Rectangular (Vertical),n/a,n/a,EN 15502-1/EN 15502-2-1,1080 kW,80/60,Nesta Plus,N 1080 FSW,https://myaic.eu/downloads,Gas - NG,Gas - LPG; G20Y20,20 mbar,865,2020,1845,39.7 mg/kWh,90-40-05/340,n/a,AIC_GasFiredCondensingBoiler,,n/a,Floor standing,Nesta Plus,N 840 FSW,N 1080 FSW,154 W,0.8 bar,17 bar,12.0 l/s,1854 W,6 bar,25 bar,,www.myaic.eu,AIC Europe BV,AIC Europe BV,Yes,,Pset_BoilerTypeCommon,IfcBoilerType,IPX4D,340.0 bar,Condensing,Stainless Steel,1758,106.6 m3/h,6.3 A,n/a,Flanged,Gas - Flange DN 80 Class PN 16,50 Hz,B23; B23p; C43; C53; C63; C83,300 mm,346.300000000000,2180.000000000000,177.900000000004,Flanged,Flange DN150 Class PN16,Fine Textured; Semi Gloss,HDG,,93%,97.41%,87.77%,0,years,Threaded,G 1"",floor-standing condensing boiler;  high modulation coefficients; combustion stability and very low NOx emissions; the high volume of heating water ensures boiler stability and maximum heat extraction; the perfect solution for any application with a high output requirement but limited plantroom space.,,info@myaic.eu,Weather compensating; Optimised Start/Stop; On/Off,Single boiler,Plain,33.4 mm,RAL 7047,750.000000000000,200.000000000000,1000.000000000000,0.000000000000,500.000000000000,200.000000000000,1,Pr_60_60_08_34,Uniclass2015,Yes,Modulating,n/a,1132.000000000000,1806.000000000000,278.000000000000,566.000000000000,2084.000000000000,1755.000000000000,465.000000000000,171.999999999999,2076.000000000000,633.000000000000,51.000000000000,102.000000000000,100.000000000000,2025.000000000000,,Yes,AIC_Boiler_Nesta_Plus_1080-1260_FSW,Fixed,n/a,300 mm,1,0,232.000000000000,325.000000000000
Nesta plus 1260 FSW,,0,www.myaic.eu,0,16,DaPr,Yes,600 liters,,info@myaic.eu,years,0,,400,www.myaic.eu,Space heating,,3,87 dB,,Rectangular (Vertical),n/a,n/a,EN 15502-1/EN 15502-2-1,1260 kW,80/60,Nesta Plus,N 1260 FSW,https://myaic.eu/downloads,Gas - NG,Gas - LPG; G20Y20,20 mbar,865,2020,1845,24.0 mg/kWh,90-40-05/340,n/a,AIC_GasFiredCondensingBoiler,,n/a,Floor standing,Nesta Plus,,N 1260 FSW,226 W,0.8 bar,17 bar,13.2 l/s,2722 W,6 bar,25 bar,,www.myaic.eu,AIC Europe BV,AIC Europe BV,Yes,,Pset_BoilerTypeCommon,IfcBoilerType,IPX4D,450.0 bar,Condensing,Stainless Steel,1850,123.6 m3/h,6.3A,n/a,Flanged,Gas - Flange DN 80 Class PN 16,50 Hz,B23; B23p; C43; C53; C63; C83,300 mm,346.300000000000,2180.000000000000,177.900000000004,Flanged,Flange DN150 Class PN16,Fine Textured; Semi Gloss,HDG,,93%,97.33%,87.72%,0,years,Threaded,G 1"",floor-standing condensing boiler;  high modulation coefficients; combustion stability and very low NOx emissions; the high volume of heating water ensures boiler stability and maximum heat extraction; the perfect solution for any application with a high output requirement but limited plantroom space.,,info@myaic.eu,Weather compensating; Optimised Start/Stop; On/Off,Single boiler,Plain,33.4 mm,RAL 7047,750.000000000000,200.000000000000,1000.000000000000,0.000000000000,500.000000000000,200.000000000000,1,Pr_60_60_08_34,Uniclass2015,Yes,Modulating,n/a,1132.000000000000,1806.000000000000,278.000000000000,566.000000000000,2084.000000000000,1755.000000000000,465.000000000000,171.999999999999,2076.000000000000,654.000000000000,51.000000000000,102.000000000000,100.000000000000,2025.000000000000,,Yes,AIC_Boiler_Nesta_Plus_1080-1260_FSW,Fixed,n/a,300 mm,1,0,232.000000000000,325.000000000000
